**OP18 Working group**

**4/9/2015**

**Agenda:**

1. **Introductions, Meeting Roles, Discussion of Agenda and Minutes of Last Meeting**
2. **HQ HVDC metering update**

1. **Generator Station Service Metering (Appendix D) Chad was going to take to MRWG**
2. **Computerized Routines for Telemeter Data Accuracy (2015 Pilot)**
3. **Remaining OP18 red-line for submission to ISO**
4. **Telemetry Full scale definitions (for Op18 definitions and appendix C change)**

ANSI/IEEE 460-1988 (lapsed): Fiducial Value - *A value to which reference is made in order to specify the accuracy of a transducer. The fiducial value is the span except for transducers have a symmetrical reversible input and output. In this case, the fiducial value is half the span.*

1. **Other topics? Technical topics from TOs for presentation or discussion.**

1. **Summation & scheduling of next face-face meeting (at ISO?)**

1. **Adjourn**